**Product Description**

**Non-woven fabric**

**Used in**

**Shoes**

* Fill the use of the sole as long as the use of the same adhesive can be.
* When used as inside, do not have to glue directly with the vamp sewn, you can achieve the effect of material saving.

**Engineering**

* The company has the production of high-density machines, can save construction time and costs.
* As long as the product covered in the soil surface, with wood stakes can be fixed to achieve soil and water conservation, to prevent the foundation emptying and other functions.
* can also be used for plant cultivation and other purposes

 **Filter area**

* Simple processing can be used.
* Applicable to automobile, motorcycle air intake, air filter ...

 **Company code**

|  |  |  |
| --- | --- | --- |
| A-class | thickness | width |
| CP-A04 | 0.4mm$\pm $0.05mm | 36" 48"72"122" |
| CP-A10 | 1.0mm$\pm $0.1mm | 36" 48"72"122" |
| CP-A30 | 3.0mm$\pm $0.1mm | 36" 48"72"122" |
| Production thickness | 0.4~3.0 mm |  |
| * This series of products are more suitable for footwear, engineering, filtration ...
 |

|  |  |  |
| --- | --- | --- |
| C-class | thickness | width |
| CP-C04 | 0.4mm$\pm $0.05mm | 36" 48"72"122" |
| CP-C10 | 1.0mm$\pm $0.1mm | 36" 48"72"122" |
| CP-C30 | 3.0mm$\pm $0.1mm | 36" 48"72"122" |
| Production thickness | 0.4~3.0 mm |  |
| * This series of products are more suitable for footwear, engineering, filtration ...
 |

|  |  |  |
| --- | --- | --- |
| E-class | thickness | width |
| CP-E04 | 0.4mm$\pm $0.05mm | 36" 48"72"122" |
| CP-E12 | 1.2mm$\pm $0.1mm | 36" 48"72"122" |
| CP-E30 | 3.0mm$\pm $0.1mm | 36" 48"72"122" |
| Production thickness | 0.4~3.0mm |  |
| * This series of products is more suitable for footwear, leather reinforcement of the material ...
 |

|  |  |  |
| --- | --- | --- |
| T-class | thickness | width |
| CP-T06 | 0.6mm$\pm $0.05mm | 36" 48"72"122" |
| CP-T10 | 1.0mm$\pm $0.1mm | 36" 48"72"122" |
| CP-T30 | 3.0mm$\pm $0.1mm | 36" 48"72"122" |
| Production thickness | 0.6~3.0mm |  |
| * This series of products is more suitable for footwear, hollow material to be filled ...
 |